,EAN##OTHER##,Nominal Wattage##ELECTRICAL_WATTAGE##WATTS,Luminous flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Color temperature##COLOR_TEMPERATURE##KELVIN,Model##OTHER##,Luminaire Length##LENGTH##MILLIMETERS,TH##OTHER##,Bracket Distance##LENGTH##MILLIMETERS,URL##OTHER##,IES Light Source##OTHER##
DP COMP 600 V 16W 840 IP66,4058075740853,16,1920,4000,DAMP PROOF COMPACT GEN 2 600 V 16W 840 IP66,600,0,400,https://www.ledvance.com/professional/search?query=4058075740853,IES_DATA_DP_COMP_G2 : DP COMP 600 V 16W 840 IP66
DP COMP 1200 V 33W 840 IP66 PS,4058075740877,33,3960,4000,DAMP PROOF COMPACT GEN 2 1200 V 33W 840 IP66 PS,1200,0,1000,https://www.ledvance.com/professional/search?query=4058075740877,IES_DATA_DP_COMP_G2 : DP COMP 1200 V 33W 840 IP66 PS
DP COMP 1500 V 50W 840 IP66 PS,4058075740891,50,6100,4000,DAMP PROOF COMPACT GEN 2 1500 V 50W 840 IP66 PS,1500,0,1300,https://www.ledvance.com/professional/search?query=4058075740891,IES_DATA_DP_COMP_G2 : DP COMP 1500 V 50W 840 IP66 PS
DP COMP TH 1200 V 33W 840 IP66 PS,4058075740914,33,3960,4000,DAMP PROOF COMPACT THROUGHWIRING GEN 2 1200 V 33W 840 IP66 PS,1200,1,1000,https://www.ledvance.com/professional/search?query=4058075740914,IES_DATA_DP_COMP_G2 : DP COMP TH 1200 V 33W 840 IP66 PS
DP COMP TH 1500 V 50W 840 IP66 PS,4058075740938,50,6100,4000,DAMP PROOF COMPACT THROUGHWIRING GEN 2 1500 V 50W 840 IP66 PS,1500,1,1300,https://www.ledvance.com/professional/search?query=4058075740938,IES_DATA_DP_COMP_G2 : DP COMP TH 1500 V 50W 840 IP66 PS
DP COMP TH 1200 V 33W 865 IP66 PS,4058075740952,33,3960,6500,DAMP PROOF COMPACT THROUGHWIRING GEN 2 1200 V 33W 865 IP66 PS,1200,1,1000,https://www.ledvance.com/professional/search?query=4058075740952,IES_DATA_DP_COMP_G2 : DP COMP TH 1200 V 33W 865 IP66 PS
DP COMP TH 1500 V 50W 865 IP66 PS,4058075740976,50,6100,6500,DAMP PROOF COMPACT THROUGHWIRING GEN 2 1500 V 50W 865 IP66 PS,1500,1,1300,https://www.ledvance.com/professional/search?query=4058075740976,IES_DATA_DP_COMP_G2 : DP COMP TH 1500 V 50W 865 IP66 PS
DP COMP TH 1500 V 62W 840 IP66,4058075740990,62,7500,4000,DAMP PROOF COMPACT THROUGHWIRING GEN 2 1500 V 62W 840 IP66,1500,1,1300,https://www.ledvance.com/professional/search?query=4058075740990,IES_DATA_DP_COMP_G2 : DP COMP TH 1500 V 62W 840 IP66
